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[image: image1.png]'SPECIFICATION for 201t 1.5.0. Stainless Steel Tank Container
Tank Type LM.O. 1., Steam Heated and Insulated.
Working Pressure 4 Bar. Nominal Capacity 24000 Litre

TYPE-CODE 124 SERIAL Nos.  ASLU 125101 to 125130
ASLU 125261 10 125336

TECHNICAL DETALS

CAPACITY (NOMINAL) 24000 Litres 6341 U.S.Gals

EXTERNAL DIMENSIONS Length 18ft- 10.5ins (6058mm)
Width 8ft- Oins (2438mm)
Height 8ft- 6ins (2591mm)

FRAME TYPE Beam

‘TARE WEIGHT (NOMINAL) 3900 Kgs.

MAXIMUM GROSS WEIGHT 30480 Kgs

PAYLOAD (NOMINAL) 26580 Kgs

STACKING HEIGHT 924000 Kgs.

TANKVESSEL  Shell material ANSI 316 stainless steel with a carbon content less
than 0.03%. Designed to ASME VIl dv. 1 pressure vessel code.
Intemai finish - mill grade 2B (32 cla). Welds longitudinal smooth
‘oven bead and circumferential ground flush and polished to 120 gri.
Single compartment with no bafles.

WORKING PRESSURE 408ar 58 p.sig.
TEST PRESSURE 608ar 87psig
MAXIMUM PRODUCT TEMPERATURE 120%
INSULATION 50 mm thick Rockwool /Foil composite mattress.
CLADDING 4 mm thick, marine grade aluminium alloy.
ACCESS Ladder and full walkway to top fitings
STEAM HEATING  Extemal steam channels welded to the tank underside o give an
SYSTEM effective surface heating area of 7 sq M
Working Pressure 6.0 Bar 87psig
Test Pressure 9.08ar 131psig

Connections are 1 inch BSP male inlet and outlet
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