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MANHOLE

AIRLINE

TOP OUTLET

BOTTOM OUTLET

DIPSTICK,

RELIEF VALVE

OTHER FITTINGS
SEALS AND
GASKETS

CUSTOM SEALS

APPROVALS

Top centally positioned, 500 mm (20 inch) dia. Stainless Steel
with SW.R. or P.T.F.Eseal, the manlid is fastened by 8-0ff s/s
swing bolts and bronze handnuts.

‘One airine nozzie with 1.5 inch ball valve fitted and terminated
With BSP capped male end, positioned at rear top of tank.

Provision only. One 3 inch flange pad fitted with a blind flange,
positioned at rear top of tank.

A 3 inch angled foot valve with remote control emergency closure,
and a 3 inch buterfly valve with a 3 inch BST'D bolted blank
flange, positioned a the rear of the tank.

A capive stainless stee! dipstick positioned at the nominal centre
of the tank within the manhole necking. The dipstick measures
the top 20% of the tanks capacity i 50 lire increments and is
used in conjuction with a calibration chart fixed adjacent to the
manway.

One 2.5 inch BSP scrawed and flanged relief valve, pressure only
(70 vacuum) with bursting disc adaplor s fitted adjacent to
manway.

One 2.5 inch flange pad fitted with a blind flange, positioned
adjacent to manway.

Allvalve and flange gaskets in contact with the cargo are P.T.F.E.

Al ftings have provision for custom seals with all fasteners.
permanentl wired to customs requirements.

LM.O. (DOT, UK) MO 1
US DOT M 101

ADR European Road Approval
RID' European Rail Approval
UIC_Intemational Rail Approval

CTC Canadian Rail Impact Tested
AAR American Association of Railfoads.
©SC Container Safety Convention
Customs Convention.
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