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150 Frame:

Tankc

‘Applcab reguatons:

Medm

Fressure rates:

Design temperature:
weighs:

Connsctons:
<2 catinet

‘Sutaos restment:

PRELIMINARY TECHNICAL SPECIFICATION
Proposal GOS511, 19-11.08, Altes Soktions Limied.

10 pieces. 150ark container beam rame ype for the ranspor of quefied gas.

"Dimensions (1CC) e (0524382521 mm )
Watervoume: 2500 Lier

Tark diametar: 2620 m

Dasign code: 'RTOD  ASME + tamp & exempton

‘el Hesa matert: Fine gainfomto stee sce EN 10028 / 54.260
UNtank ype TS0

ADRRID, DG

‘aaR.o00

IR (Transportunder Custom Seal )
(CSC (Convention of Sfe Containérs) TC impst spprovec.
USDOT4CFR

Burssu Veriss  ASMEALA.

Filrsto
Eiylene oxde and chiorotetauors-

‘atvane mixure, UN 3267 118 kgl max 28500 kg.

Eylene orde and pertatucrosthane

mixure, UN 3298 102 kgt

Einylene orde and terafucrosthane.

mixure, UN 3298 103 kgt

Nthyiamine, anhydrous, UN 1081 Lo

MAWE. 20 Bag

MAW.P.US-00T 20 Bag

Testpressure 28 Bag

ey Full vasm

Intemsl & extems g0 e

Tareweight (+-2%)  spprox. 7500 i

Max_ross weght. 34000 i

M payoac: 2050 i

Liuid ne (For Ve, S5 12 with 3 Y0 ACME couping + c3p + vent vale.
Vapourlne(Fort Vae, S5} 12 with 1% ACME coupling + o2p + ventvalve
Pressure gauge: 567960 mim gyoerne led. 140 bar
Temperstre gavge: 547080 mm 40160 C.

‘Safety Refef vabve in 55 3 FortVale wih rupture disc provsion
Nannose 'DN4ED withprovision forlevelgauge.

Intemsl cesn s dry on defvery incuding 0.8 barg overpressure withrirogen,
‘Outsice bastad SA 25 wih a 2ayer Hempei coingsystem.tank and frame whie RAL 3010,

(g raatment opsonal)

None, Opional 3 peces stainess sse.
s, Aluminium, 2.
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